# (C) Copyright 2005- ECMWF.
# Forecasting Systems with Variable Resolution

constant GRIBEXSection1Problem = 106 - section1Length ;

# used in local definition 13
transient localFlag=3 : hidden;

# 1-> 2
alias grib2LocalSectionPresent=present;
constant grib2LocalSectionNumber=30;

template mars_labeling "grib1/mars_labeling.def";

#1->2
if (stepType is "instant" ) {
  if (type is "em" || type is "es" ) {
    alias productDefinitionTemplateNumber=epsStatisticsPoint;
  } else {
    alias productDefinitionTemplateNumber=epsPoint;
  }
} else {
  if (type is "em" || type is "es" ) {
    alias productDefinitionTemplateNumber=epsStatisticsContinous;
  } else {
    alias productDefinitionTemplateNumber=epsContinous;
  }
}

unsigned[1] perturbationNumber  : dump;
alias number=perturbationNumber;
unsigned[1] numberOfForecastsInEnsemble  : dump;
alias totalNumber=numberOfForecastsInEnsemble;

unsigned[1] oceanAtmosphereCoupling : dump;

pad padding_loc30_1(3);

unsigned[4] legBaseDate  : dump ;
unsigned[2] legBaseTime : dump ;
unsigned[1] legNumber : dump ;
unsigned[4] referenceDate  : dump ;
unsigned[4] climateDateFrom  : dump ;
unsigned[4] climateDateTo  : dump;

alias local.oceanAtmosphereCoupling=oceanAtmosphereCoupling;
alias local.legBaseDate=legBaseDate ;
alias local.legBaseTime=legBaseTime ;
alias local.legNumber=legNumber ;
alias local.referenceDate=referenceDate ;
alias local.climateDateFrom=climateDateFrom ;
alias local.climateDateTo=climateDateTo;

alias mars._leg_number = legNumber;

pad padding_loc30_2(32);
