# Predefined grid 21

#position offsetSection2;
#transient section2Length=0 ;

template predefined_grid_values "grib1/grid_[gridDefinition].def";

#  NV -- number of vertical coordinate parameters
constant numberOfVerticalCoordinateValues=0 ;

constant neitherPresent = 255;

alias NV = numberOfVerticalCoordinateValues;
alias numberOfCoordinatesValues= numberOfVerticalCoordinateValues;

#  PV -- location
# (octet number)
constant pvlLocation = 255;

#  Data representation type
constant dataRepresentationType  = 0;

#  Grid definition
# (according to data representation type - octet 6 above)

# grib 1 -> 2
constant gridDefinitionTemplateNumber = 0;

# START 1/grid_definition.latitude_longitude_grid
# GRID DEFINITION latitude/longitude grid (or equidistant cylindrical)

alias numberOfPointsAlongAParallel=Ni;
alias numberOfPointsAlongAMeridian=Nj;

# Latitudes and Longitudes of the first and the last points
# Resolution and component flags

#  La1 - latitude of first grid point
meta geography.latitudeOfFirstGridPointInDegrees scale(latitudeOfFirstGridPoint,oneConstant,grib1divider,truncateDegrees) : read_only;
alias La1 = latitudeOfFirstGridPoint;

#  Lo1 - longitude of first grid point
meta geography.longitudeOfFirstGridPointInDegrees scale(longitudeOfFirstGridPoint,oneConstant,grib1divider,truncateDegrees) : read_only;
alias Lo1 = longitudeOfFirstGridPoint;

#  Resolution and component flags
constant resolutionAndComponentFlags = 128;

# Not flagbit numbers 7 to 0, while wmo is 1 to 8
constant ijDirectionIncrementGiven = 1 ;

# For grib 1 to 2
alias iDirectionIncrementGiven = ijDirectionIncrementGiven;
alias jDirectionIncrementGiven = ijDirectionIncrementGiven;
alias DiGiven = ijDirectionIncrementGiven;
alias DjGiven = ijDirectionIncrementGiven;

constant earthIsOblate = 0;
constant resolutionAndComponentFlags3 = 0;
constant resolutionAndComponentFlags4 = 0;
constant uvRelativeToGrid = 0;
constant resolutionAndComponentFlags6 = 0;
constant resolutionAndComponentFlags7 = 0;
constant resolutionAndComponentFlags8 = 0;

#  La2 - latitude of last grid point
meta geography.latitudeOfLastGridPointInDegrees scale(latitudeOfLastGridPoint,oneConstant,grib1divider,truncateDegrees) : read_only;
alias La2 = latitudeOfLastGridPoint;

#  Lo2 - longitude of last grid point
meta geography.longitudeOfLastGridPointInDegrees scale(longitudeOfLastGridPoint,oneConstant,grib1divider,truncateDegrees)  : read_only;
alias Lo2 = longitudeOfLastGridPoint;

alias Dj = jDirectionIncrement;
alias Di = iDirectionIncrement;

#  Scanning mode
constant scanningMode = 64;

# Not flagbit numbers 7 to 0, while wmo is 1 to 8
constant iScansNegatively = 0 ;
constant jScansPositively = 1 ;
constant jPointsAreConsecutive = 0;
constant iScansPositively = 1;

constant scanningMode4 = 0;
constant scanningMode5 = 0;
constant scanningMode6 = 0;
constant scanningMode7 = 0;
constant scanningMode8 = 0;

meta  geography.jDirectionIncrementInDegrees latlon_increment(ijDirectionIncrementGiven,jDirectionIncrement,
  jScansPositively,
  latitudeOfFirstGridPointInDegrees,latitudeOfLastGridPointInDegrees,
  numberOfPointsAlongAMeridian,oneConstant,grib1divider,0) : read_only;

meta  geography.iDirectionIncrementInDegrees latlon_increment(ijDirectionIncrementGiven,iDirectionIncrement,
  iScansPositively,
  longitudeOfFirstGridPointInDegrees,longitudeOfLastGridPointInDegrees,
  Ni,oneConstant,grib1divider,1)  : read_only;

alias latitudeFirstInDegrees  = latitudeOfFirstGridPointInDegrees;
alias longitudeFirstInDegrees = longitudeOfFirstGridPointInDegrees;
alias latitudeLastInDegrees   = latitudeOfLastGridPointInDegrees;
alias longitudeLastInDegrees  = longitudeOfLastGridPointInDegrees;
alias DiInDegrees             = iDirectionIncrementInDegrees;
alias DjInDegrees             = jDirectionIncrementInDegrees;

alias numberOfPoints=numberOfDataPoints;
#alias ls.valuesCount=numberOfValues;

# END 1/grid_definition.latitude_longitude_grid
constant PVPresent = 0;
constant PLPresent = 0;
constant reducedGrid =0;

# we always include the bitmap keys if a GDS is not present
constant numberOfUnusedBitsAtEndOfSection3 = 0;

# Table reference:
constant tableReference = 0;

#position offsetBeforeBitmap;
# meta bitmap gds_not_present_bitmap( missingValue,numberOfValues,
# numberOfPoints,
# latitudeOfFirstGridPoint,
# Ni,numberOfUnusedBitsAtEndOfSection3) : read_only;
