# Copyright 2005-2017 ECMWF.
#
# This software is licensed under the terms of the Apache Licence Version 2.0
# which can be obtained at http://www.apache.org/licenses/LICENSE-2.0.
# 
# In applying this licence, ECMWF does not waive the privileges and immunities granted to it by
# virtue of its status as an intergovernmental organisation nor does it submit to any jurisdiction.
#


# START 2/template.3.90 ----------------------------------------------------------------------
# TEMPLATE 3.90, Space view perspective or orthographic
include "grib2/template.3.shape_of_the_earth.def";

unsigned[4] Nx  : dump;
alias Ni  = Nx;
alias numberOfPointsAlongXAxis  = Nx;
alias geography.Nx=Nx;

unsigned[4] Ny  : dump;
alias Nj  = Ny;
alias numberOfPointsAlongYAxis  = Ny;
alias geography.Ny=Ny;

#  Lap - latitude of sub-satellite point
signed[4] latitudeOfSubSatellitePoint ;

#  Lop - longitude of sub-satellite point
signed[4] longitudeOfSubSatellitePoint ;

meta  geography.latitudeOfSubSatellitePointInDegrees   scale(latitudeOfSubSatellitePoint,one,grib3divider,truncateDegrees) : dump;
meta  geography.longitudeOfSubSatellitePointInDegrees   scale(longitudeOfSubSatellitePoint,one,grib3divider,truncateDegrees) : dump;

include "grib2/template.3.resolution_flags.def";

#  dx - apparent diameter of Earth in grid lengths, in X-direction
unsigned[4]  dx : dump;
alias geography.dx=dx;

#  dy - apparent diameter of Earth in grid lengths, in Y-direction
unsigned[4] dy  : dump;
alias geography.dy=dy;

#  Xp - X-coordinate of sub-satellite point
# (in units of 10-3 grid length expressed as an integer)
unsigned[4] Xp  : no_copy;
meta  geography.XpInGridLengths scale(Xp,one,thousand) : dump;
alias xCoordinateOfSubSatellitePoint=XpInGridLengths;

#  Yp - Y-coordinate of sub-satellite point
# (in units of 10-3 grid length expressed as an integer)
unsigned[4] Yp  : no_copy;
meta  geography.YpInGridLengths scale(Yp,one,thousand) : dump;
alias yCoordinateOfSubSatellitePoint=YpInGridLengths;

include "grib2/template.3.scanning_mode.def";

#  Orientation of the grid; i.e., the angle between the increasing Y-axis and the meridian of the sub-satellite point in the direction of increasing latitude
signed[4] orientationOfTheGrid : edition_specific;
meta geography.orientationOfTheGridInDegrees
    scale(orientationOfTheGrid,oneConstant,grib3divider,truncateDegrees) : dump; 

#  Nr - altitude of the camera from the Earth's centre, measured in units of the Earth's
# (equatorial)
unsigned[4] Nr : edition_specific,no_copy;
alias altitudeOfTheCameraFromTheEarthSCenterMeasuredInUnitsOfTheEarth = Nr;
meta geography.NrInRadiusOfEarth scale(Nr,oneConstant,oneMillionConstant,truncateDegrees) : dump;

#  Xo - X-coordinate of origin of sector image
unsigned[4] Xo  : dump;
alias xCoordinateOfOriginOfSectorImage=Xo;
alias geography.Xo=Xo;

#  Yo - Y-coordinate of origin of sector image
unsigned[4] Yo  : dump;
alias yCoordinateOfOriginOfSectorImage=Yo;
alias geography.Yo=Yo;

