Hornbeam - Case 6.3.2 : Pass - 3 ms @ 2023-08-11T05:15:10.036Z

Case Description
Send invalid UTF-8 text message in fragments of 1 octet, resulting in frames ending on positions which are not code point ends.
MESSAGE:
cebae1bdb9cf83cebcceb5eda080656469746564

Case Expectation
The connection is failed immediately, since the payload is not valid UTF-8.

Case Outcome
Actual events match at least one expected.
Expected:
{'OK': []}
Observed:
[]

Case Closing Behavior
Connection was properly closed (OK)

## Opening Handshake

    GET /runCase?case=73&agent=Hornbeam HTTP/1.1
    Host: localhost:9001
    Upgrade: websocket
    Connection: upgrade
    Sec-WebSocket-Key: 2PVTuTgpIwPZ/r7kuO5VvQ==
    Sec-WebSocket-Version: 13

    HTTP/1.1 101 Switching Protocols
    Server: AutobahnTestSuite/0.8.2-0.10.9
    X-Powered-By: AutobahnPython/0.10.9
    Upgrade: WebSocket
    Connection: Upgrade
    Sec-WebSocket-Accept: zN0/FNPovyzBeoHcDeYYov7lqdU=

## Closing Behavior

Key | Value | Description
isServer | True | True, iff I (the fuzzer) am a server, and the peer is a client.
closedByMe | False | True, iff I have initiated closing handshake (that is, did send close first).
failedByMe | False | True, iff I have failed the WS connection (i.e. due to protocol error). Failing can be either by initiating closing handshake or brutal drop TCP.
droppedByMe | False | True, iff I dropped the TCP connection.
wasClean | False | True, iff full WebSocket closing handshake was performed (close frame sent and received) _and_ the server dropped the TCP (which is its responsibility).
wasNotCleanReason | peer dropped the TCP connection without previous WebSocket closing handshake | When wasClean == False, the reason what happened.
wasServerConnectionDropTimeout | False | When we are a client, and we expected the server to drop the TCP, but that didn't happen in time, this gets True.
wasOpenHandshakeTimeout | False | When performing the opening handshake, but the peer did not finish in time, this gets True.
wasCloseHandshakeTimeout | False | When we initiated a closing handshake, but the peer did not respond in time, this gets True.
localCloseCode | None | The close code I sent in close frame (if any).
localCloseReason | None | The close reason I sent in close frame (if any).
remoteCloseCode | None | The close code the peer sent me in close frame (if any).
remoteCloseReason | None | The close reason the peer sent me in close frame (if any).

## Wire Statistics

### Octets Received by Chop Size

Chop Size | Count | Octets
183 | 1 | 183
Total | 1 | 183

### Octets Transmitted by Chop Size

Chop Size | Count | Octets
2 | 1 | 2
3 | 20 | 60
206 | 1 | 206
Total | 22 | 268

### Frames Received by Opcode

Opcode | Count
Total | 0

### Frames Transmitted by Opcode

Opcode | Count
0 | 20
1 | 1
Total | 21

## Wire Log

    000 RX OCTETS: 474554202f72756e436173653f636173653d3733266167656e743d486f726e6265616d20485454502f312e310d0a486f7374

                   3a206c6f63616c686f73743a3930 ...

    001 TX OCTETS: 485454502f312e312031303120537769746368696e672050726f746f636f6c730d0a5365727665723a204175746f6261686e

                   5465737453756974652f302e382e ...

    002 TX FRAME : OPCODE=1, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xce

    003 TX OCTETS: 0101ce

    004 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xba

    005 TX OCTETS: 0001ba

    006 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xe1

    007 TX OCTETS: 0001e1

    008 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xbd

    009 TX OCTETS: 0001bd

    010 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xb9

    011 TX OCTETS: 0001b9

    012 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xcf

    013 TX OCTETS: 0001cf

    014 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0x83

    015 TX OCTETS: 000183

    016 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xce

    017 TX OCTETS: 0001ce

    018 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xbc

    019 TX OCTETS: 0001bc

    020 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xce

    021 TX OCTETS: 0001ce

    022 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xb5

    023 TX OCTETS: 0001b5

    024 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xed

    025 TX OCTETS: 0001ed

    026 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0xa0

    027 TX OCTETS: 0001a0

    028 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0x80

    029 TX OCTETS: 000180

    030 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   e

    031 TX OCTETS: 000165

    032 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   d

    033 TX OCTETS: 000164

    034 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   i

    035 TX OCTETS: 000169

    036 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   t

    037 TX OCTETS: 000174

    038 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   e

    039 TX OCTETS: 000165

    040 TX FRAME : OPCODE=0, FIN=False, RSV=0, PAYLOAD-LEN=1, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   d

    041 TX OCTETS: 000164

    042 TX FRAME : OPCODE=0, FIN=True, RSV=0, PAYLOAD-LEN=0, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

    043 TX OCTETS: 8000

    044 FAIL CONNECTION AFTER 1.000000 sec

    045 TCP DROPPED BY PEER