Hornbeam - Case 2.10 : Pass - 66 ms @ 2023-08-11T05:15:06.774Z

Case Description
Send 10 Pings with payload.

Case Expectation
Pongs for our Pings with all the payloads. Note: This is not required by the Spec .. but we check for this behaviour anyway. Clean close with normal code.

Case Outcome
Actual events match at least one expected.
Expected:
{'OK': [('pong', u'payload-0'), ('pong', u'payload-1'), ('pong', u'payload-2'), ('pong', u'payload-3'), ('pong', u'payload-4'), ('pong', u'payload-5'), ('pong', u'payload-6'), ('pong', u'payload-7'), ('pong', u'payload-8'), ('pong', u'payload-9')]}
Observed:
[('pong', u'payload-0'), ('pong', u'payload-1'), ('pong', u'payload-2'), ('pong', u'payload-3'), ('pong', u'payload-4'), ('pong', u'payload-5'), ('pong', u'payload-6'), ('pong', u'payload-7'), ('pong', u'payload-8'), ('pong', u'payload-9')]

Case Closing Behavior
Connection was properly closed (OK)

## Opening Handshake

    GET /runCase?case=26&agent=Hornbeam HTTP/1.1
    Host: localhost:9001
    Upgrade: websocket
    Connection: upgrade
    Sec-WebSocket-Key: oOjVSKCpiwS65bO2bsZoow==
    Sec-WebSocket-Version: 13

    HTTP/1.1 101 Switching Protocols
    Server: AutobahnTestSuite/0.8.2-0.10.9
    X-Powered-By: AutobahnPython/0.10.9
    Upgrade: WebSocket
    Connection: Upgrade
    Sec-WebSocket-Accept: GB/k+PRrpMU/yfIfph6fPfT8zCU=

## Closing Behavior

Key | Value | Description
isServer | True | True, iff I (the fuzzer) am a server, and the peer is a client.
closedByMe | True | True, iff I have initiated closing handshake (that is, did send close first).
failedByMe | False | True, iff I have failed the WS connection (i.e. due to protocol error). Failing can be either by initiating closing handshake or brutal drop TCP.
droppedByMe | True | True, iff I dropped the TCP connection.
wasClean | True | True, iff full WebSocket closing handshake was performed (close frame sent and received) _and_ the server dropped the TCP (which is its responsibility).
wasNotCleanReason | None | When wasClean == False, the reason what happened.
wasServerConnectionDropTimeout | False | When we are a client, and we expected the server to drop the TCP, but that didn't happen in time, this gets True.
wasOpenHandshakeTimeout | False | When performing the opening handshake, but the peer did not finish in time, this gets True.
wasCloseHandshakeTimeout | False | When we initiated a closing handshake, but the peer did not respond in time, this gets True.
localCloseCode | 1000 | The close code I sent in close frame (if any).
localCloseReason | None | The close reason I sent in close frame (if any).
remoteCloseCode | 1000 | The close code the peer sent me in close frame (if any).
remoteCloseReason | None | The close reason the peer sent me in close frame (if any).

## Wire Statistics

### Octets Received by Chop Size

Chop Size | Count | Octets
1 | 1 | 1
8 | 1 | 8
149 | 1 | 149
183 | 1 | 183
Total | 4 | 341

### Octets Transmitted by Chop Size

Chop Size | Count | Octets
4 | 1 | 4
11 | 10 | 110
206 | 1 | 206
Total | 12 | 320

### Frames Received by Opcode

Opcode | Count
8 | 1
10 | 10
Total | 11

### Frames Transmitted by Opcode

Opcode | Count
8 | 1
9 | 10
Total | 11

## Wire Log

    000 RX OCTETS: 474554202f72756e436173653f636173653d3236266167656e743d486f726e6265616d20485454502f312e310d0a486f7374

                   3a206c6f63616c686f73743a3930 ...

    001 TX OCTETS: 485454502f312e312031303120537769746368696e672050726f746f636f6c730d0a5365727665723a204175746f6261686e

                   5465737453756974652f302e382e ...

    002 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   payload-0

    003 TX OCTETS: 89097061796c6f61642d30

    004 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   payload-1

    005 TX OCTETS: 89097061796c6f61642d31

    006 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   payload-2

    007 TX OCTETS: 89097061796c6f61642d32

    008 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   payload-3

    009 TX OCTETS: 89097061796c6f61642d33

    010 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   payload-4

    011 TX OCTETS: 89097061796c6f61642d34

    012 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   payload-5

    013 TX OCTETS: 89097061796c6f61642d35

    014 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   payload-6

    015 TX OCTETS: 89097061796c6f61642d36

    016 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   payload-7

    017 TX OCTETS: 89097061796c6f61642d37

    018 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   payload-8

    019 TX OCTETS: 89097061796c6f61642d38

    020 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   payload-9

    021 TX OCTETS: 89097061796c6f61642d39

    022 CLOSE CONNECTION AFTER 3.000000 sec

    023 RX OCTETS: 8a

    024 RX OCTETS: 89e84679059827006987271d28d88a8909b3c29b79d2bbf766d2a6b6388a89968495dee6e5ecb2f9e5f1f3a48a89908b33c5

                   e0ea4aa9ffea57e8a38a891ef0de ...

    025 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=6538343637393035

                   payload-0

    026 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3039623363323962

                   payload-1

    027 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3936383439356465

                   payload-2

    028 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3930386233336335

                   payload-3

    029 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3165663064656261

                   payload-4

    030 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=6161353334376564

                   payload-5

    031 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=6331643765646631

                   payload-6

    032 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3837333463306437

                   payload-7

    033 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3632306266313063

                   payload-8

    034 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=6436356136313361

                   payload-9

    035 TX FRAME : OPCODE=8, FIN=True, RSV=0, PAYLOAD-LEN=2, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0x03e8

    036 TX OCTETS: 880203e8

    037 RX OCTETS: 8882de7801b3dd90

    038 RX FRAME : OPCODE=8, FIN=True, RSV=0, PAYLOAD-LEN=2, MASKED=True, MASK=6465373830316233

                   0x03e8

    039 TCP DROPPED BY ME