Hornbeam - Case 2.11 : Pass - 60 ms @ 2023-08-11T05:15:06.841Z

Case Description
Send 10 Pings with payload. Send out octets in octet-wise chops.

Case Expectation
Pongs for our Pings with all the payloads. Note: This is not required by the Spec .. but we check for this behaviour anyway. Clean close with normal code.

Case Outcome
Actual events match at least one expected.
Expected:
{'OK': [('pong', u'payload-0'), ('pong', u'payload-1'), ('pong', u'payload-2'), ('pong', u'payload-3'), ('pong', u'payload-4'), ('pong', u'payload-5'), ('pong', u'payload-6'), ('pong', u'payload-7'), ('pong', u'payload-8'), ('pong', u'payload-9')]}
Observed:
[('pong', u'payload-0'), ('pong', u'payload-1'), ('pong', u'payload-2'), ('pong', u'payload-3'), ('pong', u'payload-4'), ('pong', u'payload-5'), ('pong', u'payload-6'), ('pong', u'payload-7'), ('pong', u'payload-8'), ('pong', u'payload-9')]

Case Closing Behavior
Connection was properly closed (OK)

## Opening Handshake

    GET /runCase?case=27&agent=Hornbeam HTTP/1.1
    Host: localhost:9001
    Upgrade: websocket
    Connection: upgrade
    Sec-WebSocket-Key: s7BeW6FDSWb/ojorvFJRfA==
    Sec-WebSocket-Version: 13

    HTTP/1.1 101 Switching Protocols
    Server: AutobahnTestSuite/0.8.2-0.10.9
    X-Powered-By: AutobahnPython/0.10.9
    Upgrade: WebSocket
    Connection: Upgrade
    Sec-WebSocket-Accept: 5lPf2bYFgANCjRtt5DO8pIDbrr8=

## Closing Behavior

Key | Value | Description
isServer | True | True, iff I (the fuzzer) am a server, and the peer is a client.
closedByMe | True | True, iff I have initiated closing handshake (that is, did send close first).
failedByMe | False | True, iff I have failed the WS connection (i.e. due to protocol error). Failing can be either by initiating closing handshake or brutal drop TCP.
droppedByMe | True | True, iff I dropped the TCP connection.
wasClean | True | True, iff full WebSocket closing handshake was performed (close frame sent and received) _and_ the server dropped the TCP (which is its responsibility).
wasNotCleanReason | None | When wasClean == False, the reason what happened.
wasServerConnectionDropTimeout | False | When we are a client, and we expected the server to drop the TCP, but that didn't happen in time, this gets True.
wasOpenHandshakeTimeout | False | When performing the opening handshake, but the peer did not finish in time, this gets True.
wasCloseHandshakeTimeout | False | When we initiated a closing handshake, but the peer did not respond in time, this gets True.
localCloseCode | 1000 | The close code I sent in close frame (if any).
localCloseReason | None | The close reason I sent in close frame (if any).
remoteCloseCode | 1000 | The close code the peer sent me in close frame (if any).
remoteCloseReason | None | The close reason the peer sent me in close frame (if any).

## Wire Statistics

### Octets Received by Chop Size

Chop Size | Count | Octets
1 | 6 | 6
8 | 1 | 8
14 | 6 | 84
15 | 4 | 60
183 | 1 | 183
Total | 18 | 341

### Octets Transmitted by Chop Size

Chop Size | Count | Octets
1 | 110 | 110
4 | 1 | 4
206 | 1 | 206
Total | 112 | 320

### Frames Received by Opcode

Opcode | Count
8 | 1
10 | 10
Total | 11

### Frames Transmitted by Opcode

Opcode | Count
8 | 1
9 | 10
Total | 11

## Wire Log

    000 RX OCTETS: 474554202f72756e436173653f636173653d3237266167656e743d486f726e6265616d20485454502f312e310d0a486f7374

                   3a206c6f63616c686f73743a3930 ...

    001 TX OCTETS: 485454502f312e312031303120537769746368696e672050726f746f636f6c730d0a5365727665723a204175746f6261686e

                   5465737453756974652f302e382e ...

    002 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=1, SYNC=False

                   payload-0

    003 TX OCTETS: 89

    004 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=1, SYNC=False

                   payload-1

    005 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=1, SYNC=False

                   payload-2

    006 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=1, SYNC=False

                   payload-3

    007 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=1, SYNC=False

                   payload-4

    008 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=1, SYNC=False

                   payload-5

    009 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=1, SYNC=False

                   payload-6

    010 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=1, SYNC=False

                   payload-7

    011 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=1, SYNC=False

                   payload-8

    012 TX FRAME : OPCODE=9, FIN=True, RSV=0, PAYLOAD-LEN=9, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=1, SYNC=False

                   payload-9

    013 CLOSE CONNECTION AFTER 3.000000 sec

    014 TX OCTETS: 09

    015 TX OCTETS: 70

    016 TX OCTETS: 61

    017 TX OCTETS: 79

    018 TX OCTETS: 6c

    019 TX OCTETS: 6f

    020 TX OCTETS: 61

    021 TX OCTETS: 64

    022 TX OCTETS: 2d

    023 TX OCTETS: 30

    024 TX OCTETS: 89

    025 TX OCTETS: 09

    026 TX OCTETS: 70

    027 TX OCTETS: 61

    028 RX OCTETS: 8a89e3f6675293971e3e8c97037fd3

    029 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=6533663636373532

                   payload-0

    030 TX OCTETS: 79

    031 TX OCTETS: 6c

    032 TX OCTETS: 6f

    033 TX OCTETS: 61

    034 TX OCTETS: 64

    035 TX OCTETS: 2d

    036 TX OCTETS: 31

    037 TX OCTETS: 89

    038 TX OCTETS: 09

    039 RX OCTETS: 8a

    040 TX OCTETS: 70

    041 RX OCTETS: 897e21a9cd0e40d0a11140cde04f

    042 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3765323161396364

                   payload-1

    043 TX OCTETS: 61

    044 TX OCTETS: 79

    045 TX OCTETS: 6c

    046 TX OCTETS: 6f

    047 TX OCTETS: 61

    048 TX OCTETS: 64

    049 TX OCTETS: 2d

    050 TX OCTETS: 32

    051 TX OCTETS: 89

    052 TX OCTETS: 09

    053 RX OCTETS: 8a

    054 TX OCTETS: 70

    055 RX OCTETS: 89599e2bb229ff52de36ff4f9f6b

    056 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3539396532626232

                   payload-2

    057 TX OCTETS: 61

    058 TX OCTETS: 79

    059 TX OCTETS: 6c

    060 TX OCTETS: 6f

    061 TX OCTETS: 61

    062 TX OCTETS: 64

    063 TX OCTETS: 2d

    064 TX OCTETS: 33

    065 TX OCTETS: 89

    066 TX OCTETS: 09

    067 TX OCTETS: 70

    068 RX OCTETS: 8a

    069 TX OCTETS: 61

    070 RX OCTETS: 891bb6e1c66bd798aa74d785eb28

    071 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3162623665316336

                   payload-3

    072 TX OCTETS: 79

    073 TX OCTETS: 6c

    074 TX OCTETS: 6f

    075 TX OCTETS: 61

    076 TX OCTETS: 64

    077 TX OCTETS: 2d

    078 TX OCTETS: 34

    079 TX OCTETS: 89

    080 TX OCTETS: 09

    081 RX OCTETS: 8a

    082 TX OCTETS: 70

    083 RX OCTETS: 89ce1d74e9be7c0d85a17c10c4fa

    084 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=6365316437346539

                   payload-4

    085 TX OCTETS: 61

    086 TX OCTETS: 79

    087 TX OCTETS: 6c

    088 TX OCTETS: 6f

    089 TX OCTETS: 61

    090 TX OCTETS: 64

    091 TX OCTETS: 2d

    092 TX OCTETS: 35

    093 TX OCTETS: 89

    094 TX OCTETS: 09

    095 TX OCTETS: 70

    096 TX OCTETS: 61

    097 TX OCTETS: 79

    098 TX OCTETS: 6c

    099 TX OCTETS: 6f

    100 RX OCTETS: 8a89b7675c0bc7062567d806382682

    101 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=6237363735633062

                   payload-5

    102 TX OCTETS: 61

    103 TX OCTETS: 64

    104 TX OCTETS: 2d

    105 TX OCTETS: 36

    106 TX OCTETS: 89

    107 TX OCTETS: 09

    108 TX OCTETS: 70

    109 TX OCTETS: 61

    110 TX OCTETS: 79

    111 RX OCTETS: 8a894e1a67d33e7b1ebf217b03fe78

    112 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3465316136376433

                   payload-6

    113 TX OCTETS: 6c

    114 TX OCTETS: 6f

    115 TX OCTETS: 61

    116 TX OCTETS: 64

    117 TX OCTETS: 2d

    118 TX OCTETS: 37

    119 TX OCTETS: 89

    120 TX OCTETS: 09

    121 TX OCTETS: 70

    122 TX OCTETS: 61

    123 TX OCTETS: 79

    124 RX OCTETS: 8a89a3495d64d3282408cc28394994

    125 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=6133343935643634

                   payload-7

    126 TX OCTETS: 6c

    127 TX OCTETS: 6f

    128 TX OCTETS: 61

    129 TX OCTETS: 64

    130 TX OCTETS: 2d

    131 TX OCTETS: 38

    132 TX OCTETS: 89

    133 TX OCTETS: 09

    134 RX OCTETS: 8a

    135 TX OCTETS: 70

    136 RX OCTETS: 8915444ffb652536977a252bd62d

    137 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3135343434666662

                   payload-8

    138 TX OCTETS: 61

    139 TX OCTETS: 79

    140 TX OCTETS: 6c

    141 TX OCTETS: 6f

    142 TX OCTETS: 61

    143 TX OCTETS: 64

    144 TX OCTETS: 2d

    145 TX OCTETS: 39

    146 RX OCTETS: 8a

    147 RX OCTETS: 891ee0d00a6e81a9667181b42727

    148 RX FRAME : OPCODE=10, FIN=True, RSV=0, PAYLOAD-LEN=9, MASKED=True, MASK=3165653064303061

                   payload-9

    149 TX FRAME : OPCODE=8, FIN=True, RSV=0, PAYLOAD-LEN=2, MASK=None, PAYLOAD-REPEAT-LEN=None, CHOPSIZE=None, SYNC=False

                   0x03e8

    150 TX OCTETS: 880203e8

    151 RX OCTETS: 888224985d3f2770

    152 RX FRAME : OPCODE=8, FIN=True, RSV=0, PAYLOAD-LEN=2, MASKED=True, MASK=3234393835643366

                   0x03e8

    153 TCP DROPPED BY ME